TEST REPORT TEMPLATE FOR TELEVISION MODELS

[COVER PAGE TO BE PRINTED ON TESTING LABORATORY’S COMPANY LETTERHEAD]
	
Test Report for Television [Model Number]
[Test report reference number]


Section 1: Testing Laboratory

	a) Date of test (dd/mm/yy)
	

	b) Name of testing laboratory
	

	c) Location of testing laboratory
	

	d) Name and designation of testing officer
	

	e) Name and designation of approving officer
	

	f)Type of Test Laboratory(Manufacturer's in-house testing laboratory or Third-party accredited testing laboratory):
	

	g) Country of testing laboratory
	




Section 2: Product Specification (Nameplate/Catalogue)

	a) Brand
	

	b) Phase
	Single only

	c) Model no.
	

	d) Type of television 
(E.g CRT, LCD-CCFL, LCD-Edge LED, LCD-Full LED Backlight, Plasma, OLED, etc)
	

	e) Display Resolution 
(E.g 1920 x 1080 Full HD, 1366 x768 HD Ready, SD)
	

	f) No. of Tuner
	At least one tuner

	g) Voltage (V)
	

	h) Frequency (Hz)
	

	i) Current (A)
	

	j) Rated screen aspect ratio
	

	k) Rated screen size in diagonal (inches)
	

	l) Rated screen length (mm)
	

	m) Rated screen width (mm)
	

	n) Rated screen area (L x W) (dm2)
	

	o) Overall dimensions with stand (h x w x d) mm x mm x mm 
	

	p) Overall dimensions without stand (h x w x d) mm x mm x mm
	

	q) Weight (kg) with stand
	

	r) Weight (kg) without stand
	

	s) Rated power input On-mode stated on the nameplate (W)
	

	t) Test standard adopted for rated power input 
(E.g. IEC 62087, IEC 60065)  
	

	u) Rated standby power (W)
	

	v) Year of Manufacture
	

	w) Country of origin
	

	x)  Color
	

	y) Features - Screen mirroring, Web content access, Bluetooth Compatible, Built-in camera, MHL, Built-in DVD/Blu ray player, Twin Picture, Wi-Fi certified, 3D,USB, DLNA (include where applicable) 
	




Section 3: Energy consumption test (On mode)

	a) Test standard
	IEC 62087-3:2015

	b) Video signal
	Dynamic Broadcast signal

	c) Terminal[footnoteRef:1] [1:  HDMI cable must be used. In the event that there is no HDMI terminal on the TV, other suitable terminals can be used.] 

	HDMI or otherwise stated

	d) Source
	Blu Ray / DVD disc



	
	Measured value

	e) Voltage (V)
	230+2%

	f) Frequency (Hz)
	50+2%

	g) Current (A)
	

	h) Ambient temperature (ºC)
	23+5

	i) Screen length (mm)
	

	j) Screen width (mm)
	

	k) Screen area (L x W) (mm2)
	

	l) Standard mode 
(E.g Dynamic, THX, Game, Cinema)
	The standard mode

	n) Luminance – Standard mode (cd/m2)
(at least 228 cd/m2 if 3(p) is at least 350 cd/m2)
	

	o) Brightest picture mode 
(E.g Dynamic, THX, Game, Cinema)
	The Dynamic mode (Brightest mode)

	[bookmark: _Ref128747362]p) Luminance[footnoteRef:2] (cd/m2) [2:  If the peak white luminance of the TV in brightest picture mode setting is less than 350 cd/m2, peak luminance ratio for 3(q) shall not be less than 65% of the peak white luminance of the TV in the brightest on mode configuration. 
If 3(p) is at least 350 cd/m2, peak white luminance of TV shall not be less than 228 cd/m2 in normal configuration for 3(n). ] 

[at least 350 cd/m2]
	

	q) Luminance ratio of standard mode to brightest mode
	n/p >65% 
(if 3(p) is less than 350 cd/m2)
[Refer to footnote 2]

	r) Peak luminance measuring method during standard and brightest mode (E.g. Box and outline, 3 vertical bar)
	

	s) Power saving function (E.g on, off)
	off

	t) Video aspect ratio (E.g 16:9, 4:3)
	6.3.10.6 of IEC 62087-3  active area of the video input signal fills the entire screen

	u) Display Resolution 
(E.g 1920 x 1080 Full HD, 1366 x768 HD Ready)
	

	v) Sound level (mW)
	>50mW

	w) Duration of testing (for stabilization)
	> 60mins

	x) Duration of testing (for dynamic broadcast-content video signal)
	10mins

	y) Energy Consumption On-mode at Standard mode (W)
	



Section 4: Energy consumption test (Standby mode)

	a) Test standard
	IEC 62301 2011



	
	Measured value

	b) Voltage (V)
	230+1%

	c) Frequency (Hz)
	50+1%

	d) Current (A)
	

	e) Ambient temperature (ºC)
	23+5

	f) Passive Standby Power (W)
	

	g) Procedure of testing (5.3.2 or 5.3.3 or 5.3.4 of IEC 62301:2011)
	

	h) Active Standby Power - High (W) (Put N/A if there is no such function)
	N/A if there is no such function

	i) Active Standby Power - Low (W) (Put N/A if there is no such function)
	N/A if there is no such function

	j) Procedure of testing (5.3.2 or 5.3.3 or 5.3.4 of IEC 62301:2011)
	




Section 5: Signatures

· Name and signature of testing and approving officers
· Date

Appendix A – Photos

· Colour photos showing the exterior (E.g Front, Back, Left side and Right side) of the registered model in the available finishing and colours
· Colour photos showing the connector panel
· Colour photo of the nameplate
· Colour photos of the Picture Setting for Standard and Brightest mode (E.g Picture mode, Brightness, Sharpness, etc)
· Colour photos of the video aspect ratio during the dynamic broadcast-content testing 
· Colour photos of the Equipment used (E.g Player, Cables)
· Colour photos of the how testing equipment connected to the tested television sample 

Appendix B – Schematic Drawing

· Schematic drawing clearly indicating the model’s key internal components

Appendix C – Component List

· Technical specification and description of the model’s key internal components

